{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":29,"n_cols":12,"rows_kept":29,"merged":[[1,0,7,0],[8,0,21,0],[14,1,16,1],[14,2,16,2],[14,3,16,3],[22,0,27,0],[28,0,28,11]],"flags":["formulas_cached_only"]}
[null,"机器型号","MACHINE TYPE","UNIT","JM/JK-300S/2S/LS/R2","JM/JK-450S/2S/LS/R2","JM/JK-550S/2S/LS/R2","JM/JK-850S/2S/LS/R2","JM/JK-S/2S/LS/R2","JM/JK-1200S/2S/LS/R2","JM/JK-1600S/2S/LS/R2","JM/JK-2100S/2S/LS/R2"]
["射出装置\nINJECTION UNIT","螺杆直径","Screw Diameter","mm",28,32,35,40,45,50,55,60]
[null,"射出压力","Injection Pressure","kg/cm²",1447,1280,1388,1486,1493,1552,1533,1469]
[null,"理论射出容积","Theoretical Injection Volume","cm³",68,134,153,225,285,392,570,735]
[null,"射出重量(BMC)","Max. Shot Weight(BMC1.8)","g/oz","95/3.3","187/6.6","214/7.5","315/11.1","399/14","548/19.3","798/28.1","1029/36.2"]
[null,"射出率","Injection Rate","cm³/sec",51,97,103,127,189,240,297,326]
[null,"螺杆行程","Screw stroke","mm",110,140,160,180,180,200,240,300]
[null,"螺杆转速","Screw rotation speed","rpm","0-200","0-200","0-180","0-220","0-275","0-370","0-235","0-220"]
["锁模装置\nCLAMPING UNIT","锁模力","Clamping Force","ton",30,40,55,85,100,120,160,210]
[null,"最小模厚","Min. Mold Height","mm",120,200,220,250,280,300,300,300]
[null,"开模行程","Opening Stroke","mm",180,200,200,250,280,300,300,400]
[null,"最大开模间距","Max. Opening Distance","mm",300,400,420,500,560,600,600,700]
[null,"模柱间距","Distance Between Tie Bar","mm","355x205","400x250","500x340","560x340","580x420","610x510","750x580","860x530"]
[null,"模板尺寸","Platen Size","mm","520x370","580x430","720x560","795x575","830x670","830x740","1000x810","1130x800"]
[null,"滑板尺寸","Sliding Platen Size","mm","S:350x350","S:420x396","S:500x495","S:500x545","S:580x570","S:750x600","S:810x740","S:800x840"]
[{"$nulls":4},"2S:700x350","2S:840x396","2S:1000x495","2S:1020x545","2S:1160x570","2S:1500x600","2S:1620x740","2S:1600x840"]
[{"$nulls":4},"LS:350x350","LS:420x420","LS:495x495","LS:545x545","LS:570x570","LS:600x600","LS:740x740","LS:840x840"]
[null,"料嘴中心高","Nozzle Center Height","mm","100±50","100±50","120±50","120±50","120±50","120±50","120±50","160±50"]
[null,"料嘴中心距","Nozzle Center Distance","mm",75,75,100,100,125,125,125,180]
[null,"圆盘直径","Diameter Of Rotary Table","mm",680,800,900,1000,1000,1200,1400,1500]
[null,"顶出行程","Ejector Stroke","mm",35,35,45,55,65,75,150,150]
[null,"顶出力","Ejector Force","ton",1.2,2.3,2.3,4,5.4,5.4,11,11]
["其它\nOTHERS","最大液压压力","Max. Hydraulic Pressure","kg/cm²",140,140,140,140,140,140,140,140]
[null,"油箱容量","Oil Tank Capacity","L",150,180,230,280,350,400,500,600]
[null,"电机马力","Pump Motor Power","kW",4,5.5,7.5,11,15,15,18.5,22]
[null,"电热容量","Barrel Heating Power","kW",3.5,4.2,5.4,5.4,6.3,10,12,14]
[null,"机器重量","Machine Weight","kg",1000,1800,2700,3500,4000,7000,7500,8000]
[null,"机器外形尺寸","Machine Dimensions","m","/","/","/","/","/","/","/","/"]
["备注：\n1、JM代表立式锁模，立式注射；JK代表立式锁模，水平注射；\n2、C代表C型机；ZX代表转轴；SG代表伞骨；\n3、S代表单滑；2S代表双滑；LS代表直角；R2代表双工位圆盘；R3代表三工位圆盘；\nRemarks:\n1、JM stands for vertical mold locking, vertical injection; JK stands for vertical mold locking, horizontal injection;\n2、C stands for C-type machine; ZX stands for swivel; SG stands for umbrella bone;\n3、S stands for Single Slide; 2S stands for Double Slide; LS stands for Right Angle; R2 stands for Double Position Disc; R3 stands for Triple Position Disc;"]