{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":22,"n_cols":8,"rows_kept":22,"merged":[[0,4,0,5],[0,6,0,7],[2,0,8,0],[8,4,8,5],[8,6,8,7],[9,0,14,0],[9,4,9,5],[9,6,9,7],[10,4,10,5],[10,6,10,7],[11,4,11,5],[11,6,11,7],[12,4,12,5],[12,6,12,7],[13,4,13,5],[13,6,13,7],[14,4,14,5],[14,6,14,7],[15,0,20,0],[15,4,15,5],[15,6,15,7],[16,4,16,5],[16,6,16,7],[17,4,17,5],[17,6,17,7],[18,4,18,5],[18,6,18,7],[19,4,19,5],[19,6,19,7],[20,4,20,5],[20,6,20,7],[21,0,21,7]],"flags":["formulas_cached_only"]}
[null,"机器型号","MACHINE TYPE","UNIT","JM-1200ZX",null,"JM-1600ZX"]
[null,"射台","SHOOTING PLATFORM","GROUP","A","B","A","B"]
["射出装置\nINJECTION UNIT","螺杆直径","Screw Diameter","mm",32,32,40,40]
[null,"射出压力","Injection Pressure","kg/cm²",1531,2051,1488,1488]
[null,"理论射出容积","Theoretical Injection Volume","cm³",113,129,226,226]
[null,"射出重量(PS)","Max.Shot Weight(PS)","g/oz","110/4","124/4.5","220/8","220/8"]
[null,"射出率","Injection Rate","cm³/sec",59,53,102,102]
[null,"螺杆行程","Screw stroke","mm",140,160,180,180]
[null,"螺杆转速","Screw rotation speed","rpm","0-370",null,"0-235"]
["锁模装置\nCLAMPING UNIT","锁模力","Clamping Force","ton",120,null,160]
[null,"最小模厚","Min. Mold Height","mm",200,null,200]
[null,"开模行程","Opening Stroke","mm",200,null,200]
[null,"最大开模间距","Max. Opening Distance","mm",400,null,400]
[null,"顶出行程","Ejector Stroke","mm",100,null,150]
[null,"顶出力","Ejector Force","ton",4,null,7]
["其它\nOTHERS","最大液压压力","Max. Hydraulic Pressure","kg/cm²",140,null,140]
[null,"油箱容量","Oil Tank Capacity","L",600,null,800]
[null,"电机马力","Pump Motor Power","kW","15+5.5",null,"18.5+7.5"]
[null,"电热容量","Barrel Heating Power","kW",14.5,null,17.5]
[null,"机器重量","Machine Weight","kg",10000,null,11500]
[null,"机器外形尺寸","Machine Dimensions","m","/",null,"/"]
["备注：\n1、JM代表立式锁模，立式注射；JK代表立式锁模，水平注射；\n2、C代表C型机；ZX代表转轴；SG代表伞骨；\n3、S代表单滑；2S代表双滑；LS代表直角；R2代表双工位圆盘；R3代表三工位圆盘；\nRemarks:\n1、JM stands for vertical mold locking, vertical injection; JK stands for vertical mold locking, horizontal injection;\n2、C stands for C-type machine; ZX stands for swivel; SG stands for umbrella bone;\n3、S stands for Single Slide; 2S stands for Double Slide; LS stands for Right Angle; R2 stands for Double Position Disc; R3 stands for Triple Position Disc;"]