{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":23,"n_cols":34,"rows_kept":23,"merged":[[0,4,0,5],[0,6,0,7],[0,8,0,9],[0,10,0,11],[0,12,0,13],[0,14,0,15],[0,16,0,17],[0,18,0,19],[0,20,0,21],[0,22,0,23],[0,24,0,25],[0,26,0,27],[0,28,0,29],[0,30,0,31],[0,32,0,33],[1,0,7,0],[6,4,6,5],[6,6,6,7],[6,8,6,9],[6,10,6,11],[6,12,6,13],[6,14,6,15],[6,16,6,17],[6,18,6,19],[6,20,6,21],[6,22,6,23],[6,24,6,25],[6,26,6,27],[6,28,6,29],[6,30,6,31],[6,32,6,33],[7,4,7,5],[7,6,7,7],[7,8,7,9],[7,10,7,11],[7,12,7,13],[7,14,7,15],[7,16,7,17],[7,18,7,19],[7,20,7,21],[7,22,7,23],[7,24,7,25],[7,26,7,27],[7,28,7,29],[7,30,7,31],[7,32,7,33],[8,0,15,0],[8,4,8,5],[8,6,8,7],[8,8,8,9],[8,10,8,11],[8,12,8,13],[8,14,8,15],[8,16,8,17],[8,18,8,19],[8,20,8,21],[8,22,8,23],[8,24,8,25],[8,26,8,27],[8,28,8,29],[8,30,8,31],[8,32,8,33],[9,4,9,5],[9,6,9,7],[9,8,9,9],[9,10,9,11],[9,12,9,13],[9,14,9,15],[9,16,9,17],[9,18,9,19],[9,20,9,21],[9,22,9,23],[9,24,9,25],[9,26,9,27],[9,28,9,29],[9,30,9,31],[9,32,9,33],[10,4,10,5],[10,6,10,7],[10,8,10,9],[10,10,10,11],[10,12,10,13],[10,14,10,15],[10,16,10,17],[10,18,10,19],[10,20,10,21],[10,22,10,23],[10,24,10,25],[10,26,10,27],[10,28,10,29],[10,30,10,31],[10,32,10,33],[11,4,11,5],[11,6,11,7],[11,8,11,9],[11,10,11,11],[11,12,11,13],[11,14,11,15],[11,16,11,17],[11,18,11,19],[11,20,11,21],[11,22,11,23],[11,24,11,25],[11,26,11,27],[11,28,11,29],[11,30,11,31],[11,32,11,33],[12,4,12,5],[12,6,12,7],[12,8,12,9],[12,10,12,11],[12,12,12,13],[12,14,12,15],[12,16,12,17],[12,18,12,19],[12,20,12,21],[12,22,12,23],[12,24,12,25],[12,26,12,27],[12,28,12,29],[12,30,12,31],[12,32,12,33],[13,4,13,5],[13,6,13,7],[13,8,13,9],[13,10,13,11],[13,12,13,13],[13,14,13,15],[13,16,13,17],[13,18,13,19],[13,20,13,21],[13,22,13,23],[13,24,13,25],[13,26,13,27],[13,28,13,29],[13,30,13,31],[13,32,13,33],[14,4,14,5],[14,6,14,7],[14,8,14,9],[14,10,14,11],[14,12,14,13],[14,14,14,15],[14,16,14,17],[14,18,14,19],[14,20,14,21],[14,22,14,23],[14,24,14,25],[14,26,14,27],[14,28,14,29],[14,30,14,31],[14,32,14,33],[15,4,15,5],[15,6,15,7],[15,8,15,9],[15,10,15,11],[15,12,15,13],[15,14,15,15],[15,16,15,17],[15,18,15,19],[15,20,15,21],[15,22,15,23],[15,24,15,25],[15,26,15,27],[15,28,15,29],[15,30,15,31],[15,32,15,33],[16,0,21,0],[16,4,16,5],[16,6,16,7],[16,8,16,9],[16,10,16,11],[16,12,16,13],[16,14,16,15],[16,16,16,17],[16,18,16,19],[16,20,16,21],[16,22,16,23],[16,24,16,25],[16,26,16,27],[16,28,16,29],[16,30,16,31],[16,32,16,33],[17,4,17,5],[17,6,17,7],[17,8,17,9],[17,10,17,11],[17,12,17,13],[17,14,17,15],[17,16,17,17],[17,18,17,19],[17,20,17,21],[17,22,17,23],[17,24,17,25],[17,26,17,27],[17,28,17,29],[17,30,17,31],[17,32,17,33],[18,4,18,5],[18,6,18,7],[18,8,18,9],[18,10,18,11],[18,12,18,13],[18,14,18,15],[18,16,18,17],[18,18,18,19],[18,20,18,21],[18,22,18,23],[18,24,18,25],[18,26,18,27],[18,28,18,29],[18,30,18,31],[18,32,18,33],[19,4,19,5],[19,6,19,7],[19,8,19,9],[19,10,19,11],[19,12,19,13],[19,14,19,15],[19,16,19,17],[19,18,19,19],[19,20,19,21],[19,22,19,23],[19,24,19,25],[19,26,19,27],[19,28,19,29],[19,30,19,31],[19,32,19,33],[20,4,20,5],[20,6,20,7],[20,8,20,9],[20,10,20,11],[20,12,20,13],[20,14,20,15],[20,16,20,17],[20,18,20,19],[20,20,20,21],[20,22,20,23],[20,24,20,25],[20,26,20,27],[20,28,20,29],[20,30,20,31],[20,32,20,33],[21,4,21,5],[21,6,21,7],[21,8,21,9],[21,10,21,11],[21,12,21,13],[21,14,21,15],[21,16,21,17],[21,18,21,19],[21,20,21,21],[21,22,21,23],[21,24,21,25],[21,26,21,27],[21,28,21,29],[21,30,21,31],[21,32,21,33],[22,0,22,33]],"flags":["formulas_cached_only"]}
[null,"机器型号","MACHINE TYPE","单位UNIT","JM-150",null,"JM-300",null,"JM-400",null,"JM-550",null,"JM-850",null,"JM-1000",null,"JM-1200",null,"JM-1600",null,"JM-2000",null,"JM-2500",null,"JM-3000",null,"JM-4000",null,"JM-5000",null,"JM-6000",null,"JM-7000"]
["射出装置\nINJECTION UNIT","螺杆直径","Screw Diameter","mm",22,25,25,28,28,32,32,35,35,40,40,45,45,50,50,55,55,60,65,70,75,85,80,90,90,100,95,105,100,110]
[null,"射出压力","Injection Pressure","kg/cm²",1851,1433,1815,1446,2000,1531,2051,1713,1943,1488,1890,1493,1918,1553,1855,1533,2036,1710,2326,2005,2160,1685,1903,1503,1503,1218,1560,1278,1409,1164]
[null,"理论射出容积","Theoretical Injection Volume","cm³",38,49,54,68,86,113,129,154,173,226,226,286,315,391,470,568,712,847,1376,1595,1830,2350,2080,2640,2640,3259,3890,4760,4315,5220]
[null,"射出重量(PS)","Max. Shot Weight(PS)","g/oz","37/1.3","48/1.7","53/1.9","66/2.4","84/3","110/4","124/4.5","149/5","168/6.1","220/8","220/8","279/10","307/11","380/14","455/16","547/19","688/24","818/29","1328/48","1540/56","1771/64","2270/83","2015/73","2550/93","2574/93","3187/115","3760/137","4600/168","4172/152","5049/184"]
[null,"射出率","Injection Rate","cm³/sec",26,34,42,53,46,59,53,63,78,102,116,147,149,182,150,180,155,184,136,158,200,250,245,310,465,574,450,550,496,601]
[null,"螺杆行程","Screw Stroke","mm",100,null,110,null,140,null,160,null,180,null,180,null,240,null,240,null,300,null,415,null,415,null,415,null,415,null,550,null,550]
[null,"螺杆转速","Screw Rotation Speed","rpm","0-200",null,"0-200",null,"0-200",null,"0-180",null,"0-220",null,"0-275",null,"0-370",null,"0-235",null,"0-220",null,"0-200",null,"0-240",null,"0-240",null,"0-240",null,"0-180",null,"0-180"]
["锁模装置\nCLAMPING UNIT","锁模力","Clamping Force","ton",15,null,30,null,40,null,55,null,85,null,100,null,120,null,160,null,200,null,250,null,300,null,400,null,500,null,600,null,700]
[null,"最小模厚","Min. Mold Height","mm",100,null,120,null,200,null,220,null,250,null,280,null,300,null,300,null,300,null,400,null,400,null,400,null,400,null,500,null,500]
[null,"开模行程","Opening Stroke","mm",180,null,180,null,200,null,200,null,250,null,280,null,300,null,300,null,400,null,400,null,400,null,400,null,400,null,500,null,500]
[null,"最大开模间距","Max. Opening Distance","mm",280,null,300,null,400,null,420,null,500,null,560,null,600,null,600,null,700,null,800,null,800,null,800,null,800,null,1000,null,1000]
[null,"模柱间距","Distance Between Tie Bar","mm","275x135",null,"355x205",null,"400x250",null,"500x340",null,"560x340",null,"580x420",null,"610x510",null,"750x580",null,"860x530",null,"800x530",null,"890x590",null,"890x590",null,"890x590",null,"1110x660",null,"1110x660"]
[null,"模板尺寸","Platen Size","mm","430x290",null,"520x370",null,"580x430",null,"720x560",null,"795x575",null,"830x670",null,"830x740",null,"1000x810",null,"1130x800",null,"1070x800",null,"1180x880",null,"1180x880",null,"1180x880",null,"1460x1010",null,"1460x1010"]
[null,"顶出行程","Ejector Stroke","mm",35,null,35,null,35,null,45,null,55,null,65,null,75,null,150,null,150,null,150,null,150,null,150,null,150,null,150,null,150]
[null,"顶出力","Ejector Force","ton",1.2,null,1.2,null,2.3,null,2.3,null,4,null,5.4,null,5.4,null,11,null,11,null,11,null,11,null,11,null,11,null,11,null,11]
["其它\nOTHERS","最大液压压力","Max. Hydraulic Pressure","kg/cm²",140,null,140,null,140,null,140,null,140,null,140,null,140,null,140,null,140,null,140,null,140,null,140,null,140,null,140,null,140]
[null,"油箱容量","Oil Tank Capacity","L",120,null,150,null,180,null,230,null,280,null,350,null,400,null,500,null,600,null,600,null,700,null,700,null,700,null,800,null,800]
[null,"电机马力","Pump Motor Power","kW",3,null,4,null,5.5,null,7.5,null,11,null,15,null,15,null,18.5,null,22,null,22,null,30,null,30,null,45,null,55,null,55]
[null,"电热容量","Barrel Heating Power","kW",3,null,3.5,null,4.2,null,5.4,null,5.4,null,6.3,null,10,null,12,null,14,null,16,null,17,null,17,null,17,null,20,null,20]
[null,"机器重量","Machine Weight","kg",900,null,1000,null,1500,null,2200,null,3000,null,4000,null,7000,null,7500,null,8000,null,8000,null,11000,null,12000,null,13000,null,15000,null,16000]
[null,"机器外形尺寸","Machine Dimensions","m","/",null,"/",null,"/",null,"/",null,"/",null,"/",null,"/",null,"/",null,"/",null,"/",null,"/",null,"/",null,"/",null,"/",null,"/"]
["备注：\n1、JM代表立式锁模，立式注射；JK代表立式锁模，水平注射；\n2、C代表C型机；ZX代表转轴；SG代表伞骨；\n3、S代表单滑；2S代表双滑；LS代表直角；R2代表双工位圆盘；R3代表三工位圆盘；\nRemarks:\n1、JM stands for vertical mold locking, vertical injection; JK stands for vertical mold locking, horizontal injection;\n2、C stands for C-type machine; ZX stands for swivel; SG stands for umbrella bone;\n3、S stands for Single Slide; 2S stands for Double Slide; LS stands for Right Angle; R2 stands for Double Position Disc; R3 stands for Triple Position Disc;"]